Project Design Phase-II

Solution Requirements (Functional & Non-functional)

|  |  |
| --- | --- |
| Date | 18 October 2022 |
| Project Name | Real Time River Water Monitoring and Control Systems |
| Maximum Marks | 4 Marks |

# Functional Requirements:

Following are the functional requirements of the proposed solution.

|  |  |  |
| --- | --- | --- |
| **FR No.** | **Functional Requirement (Epic)** | **Sub Requirement (Story / Sub-Task)** |
| FR-1 | User Registration | Registration through Form Registration through Gmail  Registration through product mobile UI |
| FR-2 | User Confirmation | Confirmation via Email Confirmation via OTP |
| FR-3 | Ph level detection | Ph sensor is used to monitor the water quality and the signals are send to Arduino. |
| FR-4 | Turbidity detection | Turbidity sensor TS-300B measures the turbidity (counter of suspended matter) in the wash water and the signals are send to Arduino. |
| FR-5 | Ultrasonic generator | Waves generated at regular interval times to clear algae 25% ,50%, 100% |

# Non-functional Requirements:

Following are the non-functional requirements of the proposed solution.

|  |  |  |
| --- | --- | --- |
| **FR No.** | **Non-Functional Requirement** | **Description** |
| NFR-1 | **Usability** | Efficient to use and has simple monitoring system. |
| NFR-2 | **Security** | Mobile application is secured with firewalls protection. |
| NFR-3 | **Reliability** | Real time sensor output values with future predicted data storage. 98% efficient monitoring output. Assurance for aquaculture safety |
| NFR-4 | **Performance** | Greater performance and environmentally safe model. |
| NFR-5 | **Availability** | In form of mobile UI 24 x 7 monitoring system. |
| NFR-6 | **Scalability** | Highly Scalable. It is capable to produce a best final output. |
| NFR-7 | **Stability** | It is highly stable. |
| NFR-8 | **Efficiency** | It is highly efficient and it has simple monitoring system. |